#### Back to index | # Info for kim1

#### Commodore/MOS Kim-1

Usage:
key name description
-----------------------
F1 AD address mode
F2 DA data mode
F3 RS reset
F5 GO execute from address
F6 PC program counter (hmm.. whatever)
F7 ST step (note: NMI handling for K7 missing)
ENTER + increase address
0-F hex hex digits

Known Issues:
This driver supports the backdrop image of the KIM-1, and code images in .kim format.

Generated on Tue Jul 15 11:11:04 2003