#### Back to index | # Info for mtx512

#### Memotech MTX512

Usage:
currently, the driver requires cassette images to be stored
in the following directory -
roms\mtx512
the cassette image is a flat binary image with the first 0x12 bytes being the
original mtx header and the rest being the file data.
A note about cassette naming schemes - so long as the filename of the cassette image is the same as that stored
in the header, you should be alright.
To run a tape image just type LOAD"<image name>" at the Ready Prompt.
MTX basic is pretty much a standard dialect, so you should have no problems
using it, but graphic handling etc is a bit esoteric.

Known Issues:
Improving the tape support, because at the moment it is just a hack.
Improve the TMS99x8 driver (appears the dirtyrect handling there is not
quite right)
RELCPMH Mode (CP/M Memory configuration)
support for additional roms
No Cassette Save support.
No Printer support

created on Thu Aug 16 22:55:01 2001