
NWPA Update Package Installation Instructions for NetWare v4.11

1. From the website at  http://developer.novell.com/devres/sas/certinfo.htm
   download NWPA_UP.EXE from the "Download the Update Package" link.

2. Install DOS and the CD-ROM driver on the target server machine.

3. Create the directory C:\UPDATE, then change to that directory.

4. Copy NWPA_UP.EXE to C:\UPDATE.

5. Execute NWPA_UP.EXE in the C:\UPDATE directory.

6. Delete NBI31X.NLM, NWTAPE.CDM, and NWTAPE.DDI.
							
For new NetWare v4.11 servers:
*** Note:If your server already had NetWare v4.11 installed, jump to step 7 
      of the next section "For currently installed NetWare v4.11 servers."

7. Change directory to the D:\ directory on the CD-ROM drive, if its drive 
    letter is D:

8. Enter install at the DOS command line. Proceed through the installation of
    NetWare v4.11 as usual.
    ** For Fasttrak.ham	
    **When prompted by Install to select a device driver to load, select it to 
        Fasttrak driver.
    **And now you need to swith to console mode use <ALT><ESE> before continue installation,
        and type "load c:\update\idehd.cdm",do this is to make sure that the idehd.cdm is 
        version 2.00(1998-8-5) or newer.(you can't load default idecd.cdm,by it doesn't support  	
	LBA mode addressing,and will have problems with Fasttrak driver.)
	

9. After idehd.cdm loaded,use <ALT><ESC> to switch to installation monitor,and Proceed through
    the installation of NetWare v4.11 as usual. When the installation program prompts you to edit 
    STARTUP.NCF, enter the following lines after any set parameters but 
    before any file loading, then save the file:

	load c:\update\nwpa
	load c:\update\nbi
	load c:\update\idehd.cdm

10. Remove the NetWare CD-ROM.

11. DOWN and EXIT the server.

12. Reboot the server.




For currently installed NetWare v4.11 servers:

7. Edit STARTUP.NCF and add the following lines after any set parameters
    but before any file loading:

	load c:\update\nwpa
	load c:\update\nbi
	load c:\update\idehd.cdm

    Also add subsequent line to load the Ultra33/Ultra66/FastTrak.HAM driver.

8. Boot the server

