   Windows 98, Windows 98 SE, Windows ME, Windows2000, Win XP

   Introduction:
   -------------
   This document describes the procedure to install Windows 98/98 SE/ME
   and Windows 2000 driver for Realtek RTL8139 or 8100 PCI Fast Ethernet adapter.

   Location of Windows 98/98 SE/ME Driver :   X:\\ON_board\Lan_8139_8100\win98\RTL8139.SYS
   Location of Windows 2000 Driver        :   X:\\ON_board\Lan_8139_8100\win2000\RTL8139.SYS
   Location of Windows XP Driver          :   X:\\ON_board\Lan_8139_8100\winxp\RTL8139.SYS
                                         X: your CD-ROM Drive Letter

   Installing driver procedure on Microsoft Win98/Win98 SE/Win ME/Windows2000 :
   -------------------------------------------------------------------
      Before you start with the installation process, make sure that your
      adapter should be properly installed in your PCI bus slot.
      Executing Win98/Win98 SE/Win ME/Windows2000, it will auto-detect your
      system configuration and find the adapter hardware.  ( If Win98/Win98 SE/
      Win ME/Windows2000 does not prompt that it detects the PCI Ethernet adapter,
      there must be something wrong with the RTL8139 PCI Fast Ethernet adapter
      or your system enviroment.)

      1. Ask you to select which driver you want to install, select "Driver
         from disk provided by hardware manufacturer".

      2. Insert the Realtek RTL8139 driver disk into drive A and specify
         the setup file pathname A:\WIN98 (for Windows 98/98 SE/ME) or
                                 A:\WIN2000  (for Windows 2000) .

      3. Win98/Win98 SE/Win ME/Windows2000 will appear some messages to insert
         Win98/Win98 SE/Win ME/Windows2000 system disk to complete setup step.

      4. Win98/Win98 SE/Win ME/Windows2000 will finish the other installation procedure
         automatically, then you restart the system.

