v1.1.3790.4(A012)
.sys
(1)change PHY setting model(defual) from force model to Auto model.
(2)modify HardwareUpdateDroppedInfo.
.exe
(1)Mimo-v2.0.60.8

v1.1.3790.3(A012)
.sys
(1)change pcie reg 0x12fc from 0x6700 to 0x6500
(2)set pcie reg 0x1104 to 0x568
(3)set PHY setting model(defual) from Auto model to force model.

v1.1.3790.2(A012)
.sys
(1)change pcie reg 0x12fc from 0x6500 to 0x6700

v1.1.3790.1(A012)
.sys
(1)change phy init model.
.exe
(1)Mimo-v2.0.60.7

v1.1.3790.0(A012)
.inf
(1) Add "Wake Up Capabilities" tag from INF(device properity)
.sys
(1)Add "Wake Up Capabilities" function.
(2)Add "Reconfig h/w reg by install.ini." function.
(3)Add "Reconfig device speed by install.ini.
.exe
(1)Mimo-v2.0.60.6


v1.0.3790.3(A012)
.sys
(1)When power down,then set PCIE register 0x1104 bit 10 to 1.

v1.0.3790.2(A012)
.sys
(1).fixed "L2 Wake-On-LAN fail"

v1.0.3790.1(A012)
.sys
(1).fixed "MediaType 10F/H to 100F/H can not link"

v1.0.3790.0(A012)
.sys
Creation(2006/05/23)