#### Back to index | # Info for gbcolor

#### Nintendo Gameboy Color (1998)

This is an update to the original Gameboy system that adds color capabilities as well as backwards
compatibility.

Features:
Processor: 8 MHz Z80 work alike by Sharp with two processor modes: Single (4MHz) and double (8MHz)
Video: 10, 32, or 56 on screen colors from a palette of 32000, Screen made by Sharp
Sound: 4 Channel FM stereo
Controls: 8 directional D-Pad, A, B, select, and start buttons.
Resolution: 160x144x56 colors
Sprites: 40 - 8x16, 8x8 (four color sprites-4 colors- 1 being a transparent)
Tiles: 512 on screen making use of the 16K of VRAM
Cart Size: 256KBit - 16MBit for GB compatible games. Up to 64 MBit ROM & 128 KBytes RAM for CGB
cartridges, although 32Mbit ROM / 64K RAM carts are the largest currently manufactured.
Serial port speed: 512 Kbps
Power: ~13 hours on 2 AA batteries or AC adapter.

MESS Emulation State:
???

Generated on Tue Jul 15 11:11:04 2003