
NWPA Update Package Installation Instructions for NetWare v3.1X

1. From the website at http://developer.novell.com/devres/sas/certinfo.htm
   download NWPA_UP.EXE from the "Download the Update Package" link.

2. Install DOS and the CD-ROM driver on the target server machine.

3. Create the directory C:\SERVER.312, then change to that directory.

4. Copy NWPA_UP.EXE to C:\SERVER.312.

5. Execute NWPA_UP.EXE in the C:\SERVER.312 directory.

6. Delete NBI.NLM and NWTAPE.CDM.

7. Execute 312PTD.EXE in the same directory.

For new NetWare v3.1X servers:
*** Note:If your server already had NetWare v3.1X installed, jump to step 8
       of the next section "For currently installed NetWare v3.1X servers."

8. Change directory to the D:\NETWARE.312\ENGLISH directory on the 
    CD-ROM drive, if its drive letter is D:

9. Enter install at the DOS command line. Proceed through the installation
    of NetWare v3.1X as usual, until the installation program ends with the
    cursor at the server console command line.

10. At the server console enter the following commands:
	load C:\SERVER.312 312ptc\native\start\npapatch


	load C:\SERVER.312 mmattrfx
	load C:\SERVER.312 nbi31x

11. Load the Ultra33/Ultra66/FastTrak.HAM driver.
							
12. Continue installation by loading INSTALL.NLM.

13. Create AUTOEXEC.NCF, as Install prompts you.

14. Create STARTUP.NCF, add the following lines before line "load Ultra33/Ultra66/FastTrak"
     ,then save the file:
           load c:\SERVER.312\312ptc\native\start\npapatch
           load c:\SERVER.312\mmattrfx
           load c:\SERVER.312\nbi31x

15. DOWN and EXIT the server.

16. Remove the NetWare CD-ROM.

17. Reboot the server.


For currently installed NetWare v3.1X servers:

8. Edit STARTUP.NCF and add the following lines after any set parameters
    but before any file loading:

	load c:\SERVER.312\312ptc\native\start\npapatch
	load c:\SERVER.312 \mmattrfx
	load c:\SERVER.312\nbi31x

   Also add subsequent line to load the Ultra33/Ultra66/FastTrak.HAM driver.

9. Boot the server.


