| This section lists some notes on using CD-LabelPrint. |  |
| Displaying and printing text |  |
| Depending on the font or the font size of the text used in CD-LabelPrint, the text may be printed slightly in a different position or size compared to how it was displayed. In such case, change the font and font size. |  |
| About printing |  |
| When printing a label sheet using CD-LabelPrint, it may take time depending on the printer you are using. Moreover, note that some printer drivers may create extremely large temporary files when high-quality photo images are used. |  |
| About TWAIN devices such as digital cameras |  |
| When using TWAIN-compliant devices such as digital cameras and scanners, verify that images are imported correctly with the TWAIN driver or utility software attached to the device before using CD-LabelPrint to import images. To use a TWAIN device, you need to install a driver attached to the device. For digital cameras, connection kit between the computer and the device may be sold separately. For connection methods and kits, refer to the manual of the device, or contact the manufacturer directly. CD-LabelPrint supports 32 bit TWAIN drivers. Therefore with 16 bit TWAIN drivers and TWAIN drivers not to the standard, the driver screen may not be displayed correctly, or the screen may not be imported correctly. |  |